
Children’s Product Certificate
Date of Certificate	Apr 01, 2024
[bookmark: _GoBack]Product OverviewProduct name:            Ride On  Car		
Item Number:              370-303V80PK (HLY8888)	
Date of Manufacture:  Feb 01,2024	
Manufacture:  
PINGHU SHUANGXI BABY CARRIER MANUFACTURE CO.,LTD
Address of Manufacture: 
XINCANG TOWN, PINGHU CITY, ZHEJIANG PROVINCE, CHINA 
Imported By:                  Aosom LLC  
		            27150 SW Kinsman Rd
            Wilsonville, OR 97070
            T: 503.746.5886
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      Product Reference Image 		


Testing and Records OverviewAosom LLC
27150 SW Kinsman Rd
Wilsonville, OR 97070
Corey Shull
T: 503.746.5886
Bureau Veritas Testing Technical Service (Zhejiang) Co.,Ltd
1F west, 6F east, 7F east, 8F, Building B,No.66,Qingyi Road, Ningbo, Zhejiang, China
Tel.: 86-574-87091330                                            Mail: allen.he@bureauveritas.com Web:www.cps.bureauveritas.com
Test Location and Contact Information
Test Date: Feb 22,2024

Certification Issued and Test Records Maintained By

Aosom LLC certifies that the above product complies with the following rules, banes, regulations and standards:   
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4.25

Battery-operated Toys—These requirements are i tended to address potential

risks of injury associated with batlery usage in foys

(for example, battery

overheating, leakage. explosion and fire, and choking on or swallowing

batteries)

4251

The toy shall be marked permanently on the
battery compartment or on the area immediately
adjacent to the battery compartment to show the
correct battery polarity using the

polarity symbols “+” and °~". Additional markings
located on the toy o in the instructions shall
indicate the correct batlery size and voltage.
These markings are not required for non-
replaceable bateries or secondary batteries that,
by design, can only be inserted in the correct
orientation. Battery compartments for button cell
or coin cell batteries are not subject to this
requirementf itis not practicable to mark the
battery compartment due to size limitations or
other considerations: in such instances, markings
required by this section shall be in the
instructions

N OTE 14—The battery compartment door is
considered part of the battery compartment.
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5.14

Battery-operated Toys—Toys with non-
replaceable batteries that are accessible with the
use of a coin, screwdriver, or other common
household tool shall bear a statement that the
battery is not replaceable. If the manufacturer
determines that it is impractical to label the
product, this information shall be placed on the
packaging or in the instructions.
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5.3

Safety Labeling Requirements—Certain toys, and
in some cases their packaging or their
instructions, or both, are required to carry safety
labeling to comply with this specification.
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TEST REQUESTED CONCLUSION
The mechanical hazards requirements of ASTM F963-23, “Standard consumer safety PASS
specification for toy safety.(Excluding clause 4.25)

The labeling requirements of ASTM F963-23, “Standard consumer safety specification for toy PASS
safety.(Excluding clause 5.14.185.3)

The flammability requirement of solids under ASTM F963-23 section 4.2 according to Annex A5, PASS
"Flammability testing procedure for solids and soft toys"

The Tracking Label Requirement of The Consumer Product Safety Improvement Act (CPSIA) of PASS
2008 Section 103 Tracking Labels for Children's Products

Total Lead Content in Surface Coating — United States Consumer Product Safety Improvement PASS
Act (CPSIA), Section 101(a)(2)

Phthalates Content - Reference to California Proposition 65 List of Chemicals & As Client's PASS
requirement

Phthalates Content in Children's Toys and Child Care Articles - United States Code of Federal PASS
Regulations (CFR), Title 16, Part 1307

Soluble Heavy Metals Content in Substrate - ASTM International Standard ASTM F963-23, PASS
Section 4.3.5.2(2)(b)

Total Lead Content in Substrate - United States Consumer Product Safety Improvement Act PASS
(CPSIA) Section 101(a)(2)

Total Lead Content in Surface Coating- Reference to California Proposition 65 List of Chemicals PASS
& As Client’s requirement

Total Lead Content in Substrate - Reference to California Proposition 65 List of Chemicals & As PASS
Client's requirement

The total lead content of 90 ppmrequirements of 16 CFR 1303, “Ban of lead-containing paint

and certain consumer products bearing lead-containing paint” as mandated by Congress in PASS

section 101(f) of the Consumer Products Safety Improvement Act (CPSIA) of 2008, Public Law
110-314
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Total Lead in Surface Coating - ASTM International Standard ASTM F963-23, Section 4.3.5.1(1)

for Total Lead Content in Surface Coating PASS
Soluble Heavy Metals Content in Surface Coating - ASTM International Standard ASTM F963- PASS
23, Section 4.3.5.1(2)

Total Lead in Substrate Material - ASTM International Standard ASTM F963-23, Section PASS

4.3.5.2(1) for Total Lead Content in Substrate Material





