
Children’s Product Certificate
Date of Certificate	March 06, 2024
[bookmark: _GoBack]Product OverviewProduct name:           Electric Ride-on Car	
Item Number:            370-150RD/JC111A
Date of Manufacture:  2024-01-19	
Manufacture:  	PINGHU XH CHILDREN PRODUCTS CO., LTD
Address of Manufacture: NO.186, TONGCHE TOWN ROAD, XINCANG TOWN, PINGHU CITY, ZHEJIANG PROVINCE
Imported By:                  Aosom LLC  
		            27150 SW Kinsman Rd
            Wilsonville, OR 97070
            T: 503.746.5886
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      Product Reference Image 		


Testing and Records OverviewBureau Veritas Testing Technical Service(Zhejiang) Co., Ltd
1F west, 6F east, 8F, Building B, No.66, Qingyi Road, Ningbo, Zhejiang, China
Cps.bureauveritas.com


Aosom LLC
27150 SW Kinsman Rd
Wilsonville, OR 97070
Corey Shull
T: 503.746.5886
Certification Issued and Test Records Maintained By

Aosom LLC certifies that the above product complies with the following rules, banes, regulations and standards:Test Location and Contact Information
Test Date: Jan 19, 2024---Mar 06, 2024
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TEST REQUESTED [TEST METHOD/REGULATION RESULT
Phthalates Content [ASTM F063-23 AF: Pass
Flammabilty of Toys [ASTM F063-23 AE: Pass
Heavy Metals [ASTM F063-23 AF: Pass
Physical and Mechanical Hazards [ASTM F063-23 AE: Pass
Total Lead Content in Substrate US CPSIA, Section 101 AF: Pass
Phthalates Content US CPSIA, Section 108 AF: Pass
Total Lead Contentin Paint/ Surface Coafing US CPSIA, Section 101 AF: Pass
Phthalates Content [CPSC 16 CFR part 1307 AF: Pass
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