
Children’s Product Certificate
Date of Certificate	March 27, 2024
Product OverviewProduct name:           Motor bike	
Item Number:            370-188V80YL/JC916
Date of Manufacture:  2024-03-26	
Manufacture:  Pinghu XH Children Products Co., Ltd	
Address of Manufacture: No. 186 Tongche Road, Pinghu City, Zhejiang Province, China
Imported By:                  Aosom LLC  
		            27150 SW Kinsman Rd
            Wilsonville, OR 97070
            T: 503.746.5886
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      Product Reference Image 		


Testing and Records OverviewBureau Veritas Testing Technical Service(Zhejiang) Co., Ltd
1F west, 6F east, 8F, Building B, No.66, Qingyi Road, Ningbo, Zhejiang, China
Cps.bureauveritas.com
Eurofins MTS Consumer Product Testing (Shanghai) Co., Ltd. 
No.105, Guangzhong Road, Minhang, Shanghai, China


Test Date: Jan 30, 2024---Mar 27, 2024
                  Jan 29, 2024---May 22, 2024


Aosom LLC
27150 SW Kinsman Rd
Wilsonville, OR 97070
Corey Shull
T: 503.746.5886
Email: corey@aosom.com
Certification Issued and Test Records Maintained By

Aosom LLC certifies that the above product complies with the following rules, banes, regulations and standards:
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TEST REQUESTED TEST METHOD/REGULATION RESULT
Mechanical and Physical Properties ASTM F963-23 A: Pass
Flammability of Toys ASTM F963-23 A: Pass
Heavy Metals ASTM F963-23 Pass
Phthalates Content ASTM F963-23 Pass
Total Lead Content in Substrate US CPSIA, Section 101 Pass
Phthalates Content US CPSIA, Section 108 Pass
Total Lead Content in Paint / Surface Coating US CPSIA, Section 101 Pass
Phthalates Content CPSC 16 CFR part 1307 Pass
Tracking Label Assessment US CPSIA, Section 103 A: Pass





