
Children’s Product Certificate
Date of Certificate	May 27, 2024
Product OverviewProduct name:           Electric Ride-on Car	
Item Number:            370-189V80BK/JC913
Date of Manufacture:  2024-05-30	
Manufacture:  Chizhou JC Children Products Co., Ltd	
Address of Manufacture: Matang industrial zone, Dingqiao town, Qingyang district, Chizhou city, Auhui province
Imported By:                  Aosom LLC  
		            27150 SW Kinsman Rd
            Wilsonville, OR 97070
            T: 503.746.5886
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      Product Reference Image 		


Testing and Records OverviewBureau Veritas Testing Technical Service(Zhejiang) Co., Ltd
1F west, 6F east, 8F, Building B, No.66, Qingyi Road, Ningbo, Zhejiang, China
Cps.bureauveritas.com
Eurofins MTS Consumer Product Testing (Shanghai) Co., Ltd. 
No.105, Guangzhong Road, Minhang, Shanghai, China


Test Date: Jan 30, 2024---Mar 27, 2024
                  Jan 31, 2024---May 28, 2024


Aosom LLC
27150 SW Kinsman Rd
Wilsonville, OR 97070
Corey Shull
T: 503.746.5886
Certification Issued and Test Records Maintained By

Aosom LLC certifies that the above product complies with the following rules, banes, regulations and standards:
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ASTM Fo63-23

Clause

Requirement — Test

Result — Remark.

Verdict

4.25

Battery-operated Toys—These requirements are in tended (o address potential

4251

‘The toy shall be marked permanently on the
battery compartment or on the area immediately
adjacent to the battery compartment to show the
correct battery polarity using the

polarity symbols “+” and °~". Additional markings
located on the toy or in the instructions shall
indicate the correct battery size and voltage.
‘These markings are not required for non-
replaceable batteries or secondary batteries that,
by design, can only be inserted in the correct
orientation. Battery compartments for button cell
or coin cell batteries are not subject to this
requirement i it is not practicable to mark the
battery compartment due to size limitations or
other considerations; in such instances, markings
required by this section shall be in the
instructions.

N OTE 14—The battery compartment door is.
considered part of the battery compartment.

42511

Toys containing non-replaceable batteries shall
be labeled in accordance with 5.14.

4252

The maximum allowable direct current potential
between any two accessible electrical points
24V nominal

DC 6V<24v
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TEST REQUESTED TEST METHOD/REGULATION __|RESULT
Mechanical and Physical Properties. [ASTM F963-23 A Pass
Flammabilty of Toys [ASTM F963-23 A Pass
Heavy Metals [ASTM F963-23 Pass
Phthalates Content [ASTM F963-23 Pass
Total Lead Content in Substrate US CPSIA, Section 101 Pass
Phthalates Content US CPSIA, Section 108 Pass
Total Lead Content in Paint/ Surface Coating US CPSIA, Section 101 Pass
Phthalates Content CPSC 16 CFR part 1307 Pass
Tracking Label Assessment US CPSIA, Section 103 A Pass





