
[bookmark: _GoBack]Children’s Product Certificate
Date of Certificate	May 24, 2024
Product OverviewProduct name:           Electric Ride-on Car	
Item Number:            370-260V80PK/JC915
Date of Manufacture:  2024-01-30	
Manufacture:  Chizhou JC Children Products Co., Ltd	
Address of Manufacture: Matang industrial zone, Dingqiao town, Qingyang district, Chizhou city, Auhui province
Imported By:                  Aosom LLC  
		            27150 SW Kinsman Rd
            Wilsonville, OR 97070
            T: 503.746.5886
[image: IMG_3698]

	
		
		
	


      Product Reference Image 		


Testing and Records OverviewBureau Veritas Testing Technical Service(Zhejiang) Co., Ltd
1F west, 6F east, 8F, Building B, No.66, Qingyi Road, Ningbo, Zhejiang, China
Cps.bureauveritas.com
Eurofins MTS Consumer Product Testing (Shanghai) Co., Ltd. 
No.105, Guangzhong Road, Minhang, Shanghai, China


Test Date: Jan 30, 2024---Apr 24, 2024
                  Feb 02, 2024---May 13, 2024


Aosom LLC
27150 SW Kinsman Rd
Wilsonville, OR 97070
Corey Shull
T: 503.746.5886
Certification Issued and Test Records Maintained By

Aosom LLC certifies that the above product complies with the following rules, banes, regulations and standards:
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TEST REQUESTED TEST METHOD/REGULATION RESULT
Phthalates Content ASTM F963-23 Pass
Flammability of Toys ASTM F963-23 A: Pass
Heavy Metals ASTM F963-23 Pass
Mechanical and Physical Properties ASTM F963-23 A: Pass
Total Lead Content in Substrate US CPSIA, Section 101 Pass
Phthalates Content US CPSIA, Section 108 Pass
Total Lead Content in Paint / Surface Coating US CPSIA, Section 101 Pass
Phthalates Content CPSC 16 CFR part 1307 Pass
Tracking Label Assessment US CPSIA, Section 103 A: Pass
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ASTM F963-23

Clause

Requirement  Test

Result— Remark.

Verdict

4.25

Batlery-operated Toys—These requirements are in tended to address potential

isks of injury associated with battery usage in toys

(for example, battery

overheating, leakage, explosion and fire, and choking on or swallowing

batteries)

4251

The toy shall be marked permanently on the
battery compartment or on the area immediately
adjacent to the battery compartment fo show the
correct battery polarity using the

polarity symbols “+” and °~"_ Addtional markings
located on the toy o in the instructions shall
indicate the correct battery size and voltage.
These markings are not required for non-
replaceable batteries or secondary batteries that,
by design, can only be inserted in the correct
orientation. Battery compartments for button cel
or coin cell batteries are not subject to this
requirementf itis not practicable to mark the
battery compartment due to size limitations or
other considerations: in such instances, markings
required by this section shall be in the
instructions

N OTE 14—The battery compartment door is
considered part of the battery compartment.

42511

Toys containing non-replaceable batteries shall
be labeled in accordance with 5.14.

4252

The maximum allowable direct current potential
between any two accessible electrical points is
24 V nominal

DC 12v<24V.
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Baliery-operated oys shall bo designed sotral
s not possibe to charge any nonrechargeatie:
[battry. This can be achieved trough prysical
|desig ofthe battery compartment r thrcugh the
[use of an approprat eleckical crcuit

[design. Tris applie tosiaonsin which a
[bttry may be nstaed incorrecty (reversec) or
i wicha battery charger may be applied 03 oy
|containig non-rechargeable batedes,r balh

[T section does not apoy to rcuts having one.
oo nan-rechargeable battries as e oy
|source o powe.

AT

Toys having a Groul powered oy by Bulion GoT
type battories are not subjecttotis requirement.

rExy

‘aery Acoassbiny—Batiry acoessibaty befos|
Jan atertostng in acordance with 85 —8.10
|sha b cetermined n sccordance wih 4.25.4.1
lor 425 42, 2s appicable Testing s poformed
Jusing the recommendod batteies nstaiod.

4241

For bys iended forchidren less fan 3 years
|0 no battery sha be accossse wihout
[requiig the use of a common housahad tool o
|acoess te bateryges).

[a7-72mantrs

ez

[For al oys tratutze bateres wheh il
|completely witin e small paris test cyinder
[shown i Fig. 3 such bateries sha nt be
laccessile without requirg e use

o comman housenald o 1o access the.
battoros)

A

2 siener 5 (ad o sacrs e Eatery
|compatment i shal remain attached o e toy
o batry compartment cover, before ad after
tesing i accordance with 85 ~8.10

T

‘Asan atermatve (o common housenol 3.
I manufacturers are pernited fo doc b uso @
|specaty fastener (o exampie, Tox. Hex) to
[secure the batery comparimert, i acoordance

[ Wit o requirements o 425 4, e appropriate
oo i included wih e toy. and instrucional
|material conforming 1 6.9 is included.





