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CHILDREN’S PRODUCT CERTIFICATE(CPC)


	Us Importer/Domestic Manufacturer
	Person Maintaining Records

	Aosom LLC
	Aosom LLC

	27150 SW Kinsman Rd,Wilsonville,OR 97070 Corey Shull
	27150 SW Kinsman Rd,Wilsonville,OR 97070 Corey Shull

	Tel No.: 503.746.5886
	Tel No.: 503.746.5886

	Email: Zhang.vito@gmail.com
	Email: Zhang.vito@gmail.com



	Sample Description:
	KID'S SLIDE

	Color:
	colorful

	Style No(S).:
	LY-2015

	Manufacturer:
	LIYOU INDUSTRIAL CO., LTD

	Date Of Manufacture:
	Dec. 2025

	Place Of Manufacture:
	YANGWAN INDUSTRIAL ZONE QIAOXIA TOWN YONGJIA COUNTY,ZHEJIANG,CHINA



	Testing Lab:
	Intertek Testing Services Ltd .Zhejiang, Ningbo Branch

	Address:
	4F's Area 2-3 , 5F, No.6 Building,Lingyun Industry Park, No.1177 Lingyun Road, Ningbo National Hi-Tech Zone, Ningbo,China,315000

	Contact Person: Jim
	Tel: : +86 574 87137200

	Test Report No.:
	SHAH01879292，SHAH0188113601
	Date of Testing:
	Dec.,2025

	Place of Testing:
	Ningbo,China 



	The following rules, bans, standards and regulations were tested for this product:

	1 
	ASTM F963-23 Standard Consumer Safety Specification for Toy Safety

	2 
	U.S. ASTM F963-23 Flammability Test of Materials other than Textile Materials

	3 
	U.S. ASTM F963-23 Section 4.3.5.1(2) and 4.3.5.2(2) on Soluble Elements Content

	4 
	U.S. ASTM F963-23 Section 4.3.5.2(2) on Total Lead Content in Non-surface Coating Materials

	5 
	U.S. Consumer Product Safety Improvement Act 2008 title I, section 101 for total Lead content in non-surface coating materials (substrate)

	6 
	US Consumer Product Safety Improvement Act 2008 Title I, Sec 108(a) & (b)(3) and US 16 CFR Part 1307 for Prohibition of Children’s Toys and Child Care Articles Containing Specified Phthalates

	7 
	ASTM F963-23 Section 4.3.8 on Phthalates Content

	8 
	Consumer Product Safety Act section 14(a)(5) tracking labels for Children Products

	9 
	U.S. ASTM F963-23 Section 4.3.5.1 on Soluble Elements Content in Surface Coating

	10 
	U.S. ASTM F963-23 Section 4.3.5.1 on Total Lead Content in Surface 
Coating
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