
Children’s Product Certificate
Date of Certificate	APR 28,2024[image: ]

Product OverviewProduct name:     BABY RIDE ON CAR 	
Item Number:     370-116PK         	
Date of Manufacture:  Jul 2,2024	
Manufacture:  	NINGBO PRINCE TOYS CO.,LTD.
Address of Manufacture: NO.777 EAST TAOYUAN ROAD,GUANHAIWEI TOWN,CIXI CITY,ZHEJIANG,CHINA
Imported By:                  Aosom LLC  
		            27150 SW Kinsman Rd
            Wilsonville, OR 97070
            T: 503.746.5886

	
		
		
	


      Product Reference Image 		

[bookmark: _GoBack]Testing and Records OverviewBureau Veritas Testing Technical Service (Zhejiang) Co.,Ltd
1F west,6F east,7F east,8F,Building B,No.66,Qingyi Road,Ningbo,Zhejiang,China
Tel:86-574-87091333,Fax:86-574-87971038
website:cps.bureauveritas.com

Aosom LLC
27150 SW Kinsman Rd
Wilsonville, OR 97070
Corey Shull
T: 503.746.5886
Certification Issued and Test Records Maintained By

Aosom LLC certifies that the above product complies with the following rules, banes, regulations and standards:  Test Location and Contact Information
Test Date: APR 9,2024
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EXECUTIVE SUMMARY:

TEST REQUESTED CONCLUSION
The mechanical hazards requirements of ASTM F963-23, “Standard consumer safety PASS
specification for toy safety.

Tn;e :abeling requirements of ASTM F963-23, “Standard consumer safety specification for toy PASS
safety.

The flammability requirement of solids under ASTM F963-23 section 4.2 according to Annex A5, PASS
"Flammability testing procedure for solids and soft toys"
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EXECUTIVE SUMMARY:

TEST REQUESTED CONCLUSION
Total Lead Content in Surface Coating — United States Consumer Product Safety Improvement PASS
Act (CPSIA), Section 101(a)(2)

Phthalates Content in Children’s Toys and Child Care Articles - United States Code of Federal PASS
Regulations (CFR), Title 16, Part 1307

Total Lead Content in Substrate - United States Consumer Product Safety Improvement Act PASS
(CPSIA) Section 101(a)(2)

Soluble Heavy Metals Content in Substrate - ASTM International Standard ASTM F963-23, PASS
Section 4.3.5.2(2)(b)

Total Heavy Metals Content - Initial Screening of ASTM International Standard ASTM F963-23, PASS
Section 4.3.5.2(2)(b) for Soluble Heavy Metals Content in Substrate

Total Lead in Surface Coating - ASTM International Standard ASTM F963-23, Section 4.3.5.1(1) PASS
for Total Lead Content in Surface Coating

Soluble Heavy Metals Content in Surface Coating - ASTM International Standard ASTM F963- PASS
23, Section 4.3.5.1(2)

Total Lead in Substrate Material - ASTM International Standard ASTM F963-23, Section PASS

4.3.5.2(1) for Total Lead Content in Substrate Material





