
Children’s Product Certificate
Date of Certificate	Apr 8，2026[image: ]


Product OverviewProduct name:     BABY RIDE ON CAR 	
Item Number:     370-441V00BK （667）  	
Date of Manufacture: Apr 8，2026	
Manufacture:  	NINGBO PRINCE TOYS CO.,LTD.
Address of Manufacture: NO.777 EAST TAOYUAN ROAD,GUANHAIWEI TOWN,CIXI CITY,ZHEJIANG,CHINA
Imported By:                  Aosom LLC  
		           7777 Center Ave. Suite 430
           Huntington Beach, CA 92647-9998 USA
    

	
		
		
	


      Product Reference Image 		

Testing and Records OverviewBureau Veritas Testing Technical Service
(Zhejiang) Co.,Ltd
1F west, 6F east, 7F east, 8F, Building B,
No.66,Qingyi Road, Ningbo, Zhejiang, China
Tel:86-574-87091333
llyli.li@bureauveritas.com
Aosom LLC
7777 Center Ave. Suite 430
Huntington Beach, CA 92647-9998 USA
Email:corey@aosom.com
Corey Shull
Certification Issued and Test Records Maintained By

Aosom LLC certifies that the above product complies with the following rules, banes, regulations and standards:  Test Location and Contact Information
Test Date: Mar  17,2025
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TEST REQUESTED CONCLUSION
Phthalates Content in Children's Toys and Child Care Arficies - United States Code of Federal PASS
Regulations (CFR), Title 16, Part 1307

Total Lead Content in Surface Coating — United States Consumer Product Safety Improvement oASS
Act (CPSIA), Section 101(a)(2)

Total Lead Content in Substrate - United States Consumer Product Safety Improvement Act oASS
(CPSIA) Section 101(a)(2)

“The total lead content of 90ppm requirements of 16 CFR 1303, “Ban of lead-containing paint

and certain consumer products bearing lead-containing paint’ as mandated by Congress in PASS
section 101(7) of the Consumer Products Safety Improvement Act (CPSIA) of 2008, Public Law

110-314.

Phthalates Content- ASTM International Standard ASTM F963-23, Section 4.3.8 for Phthalates PASS
Soluble Heavy Metals Content in Substrate - ASTM Intemational Standard ASTM F963-23, PASS
Section 4.3.5.2(2)(b)

Total Lead in Surface Coating - ASTM International Standard ASTM F963-23, Section 4.3.5.1(1) PASS
for Total Lead Content in Surface Coating

‘Soluble Heavy Metals Content in Surface Coating - ASTM Intemational Standard ASTM F963- PASS
23, Section 4.35.1(2)

Total Lead in Substrate Material - ASTM International Standard ASTM F963-23, Section PASS

4.3.5.2(1) for Total Lead Content in Substrate
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TEST REQUESTED CONCLUSION

The mechanical hazards requirements of ASTM F963-23, “Standard consumer safety PASS
specification for toy safety.

The labeling requirements of ASTM F963-23, “Standard consumer safety specification for toy PASS
safety.

The flammability requirement of solids under ASTM F963-23 section 4.2 according to Annex A5,

"Flammability testing procedure for solids and soft toys" PASS





